From 22f37d07d12714990714ecd32dd0d63ec644c734 Mon Sep 17 00:00:00 2001
From: Leah Rowe <info@minifree.org>
Date: Mon, 12 Aug 2024 02:15:24 +0100
Subject: [PATCH 10/18] nb/x4x: define INTEL_GMA_DPLL_REF_FREQ

set it to 96MHz. fixes the following build error when
building for x4x boards e.g. gigabyte ga-g41m-es2l:

hw-gfx-gma-plls.adb:465:46: error: "INTEL_GMA_DPLL_REF_FREQ" not declared in "Config"
make: *** [Makefile:423: build/ramstage/libgfxinit/common/g45/hw-gfx-gma-plls.o] Error 1

this error was introduced when merging coreboot/dell
into coreboot/default in lbmk. nicholas chin's fix in lbmk
was as follows:

commit 8629873a6043067affc137be275b7aa69cb1f10c
Author: Nicholas Chin <nic.c3.14@gmail.com>
Date:   Mon May 20 10:46:25 2024 -0600

    Fix E6400 display issue with 1440 x 900 panel

this currently corresponds to the patch in lbmk,
as of 12 august 2024:

0042-mb-dell-e6400-Use-100-MHz-reference-clock-for-displa.patch

The assumption prior to Nicholas's fix was 96MHz, so set
it accordingly on x4x northbridge.

Signed-off-by: Leah Rowe <info@minifree.org>
---
 src/northbridge/intel/x4x/Kconfig | 4 ++++
 1 file changed, 4 insertions(+)

diff --git a/src/northbridge/intel/x4x/Kconfig b/src/northbridge/intel/x4x/Kconfig
index 9af063819b..93ba575b95 100644
--- a/src/northbridge/intel/x4x/Kconfig
+++ b/src/northbridge/intel/x4x/Kconfig
@@ -14,6 +14,10 @@ config NORTHBRIDGE_INTEL_X4X
 
 if NORTHBRIDGE_INTEL_X4X
 
+config INTEL_GMA_DPLL_REF_FREQ
+	int
+	default 96000000
+
 config CBFS_SIZE
 	default 0x100000 if !SOUTHBRIDGE_INTEL_I82801GX
 
-- 
2.39.5

