From f8eb43796090965baef1c6f75aa438e2918bf2e1 Mon Sep 17 00:00:00 2001
From: Leah Rowe <leah@libreboot.org>
Date: Fri, 7 May 2021 19:43:32 +0100
Subject: [PATCH 03/10] asus/kgpe-d16: enable lc_cache_partitioning and
 experimental_memory_speed_boost

This really only benefits 63xx opterons which are less reliable in libreboot due
to lack of CPU microcode updates, but we might aswell enable this anyway.
---
 src/mainboard/asus/kgpe-d16/cmos.default | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/src/mainboard/asus/kgpe-d16/cmos.default b/src/mainboard/asus/kgpe-d16/cmos.default
index 7c496a50d7..8a25620e1d 100644
--- a/src/mainboard/asus/kgpe-d16/cmos.default
+++ b/src/mainboard/asus/kgpe-d16/cmos.default
@@ -21,10 +21,10 @@ sata_ahci_mode=Enable
 sata_alpm=Disable
 maximum_p_state_limit=0xf
 probe_filter=Auto
-l3_cache_partitioning=Disable
+l3_cache_partitioning=Enable
 ieee1394_controller=Enable
 gart=Enable
 ehci_async_data_cache=Enable
-experimental_memory_speed_boost=Disable
+experimental_memory_speed_boost=Enable
 power_on_after_fail=On
 boot_option=Fallback
-- 
2.39.2

